miim

### MLB-094 Remote auto interlock not engaged

The command to select automatic mode has been executed but the remote auto hardware interlock is not engaged.

As a result, the command is not executed.

What you should do:

1. Determine the cause of the problem.

Either correct the program or engage the remote auto interlock. Manually select AUTO mode to continue the measurement routine.

2. If the error is supposed to support this operation:

   If the error reoccurs, contact your Giddings & Lewis service representative.