miim

### Installation Information

Before you install PC-DMIS, configure your portlock or LMS license for the HP-C-Ve interface. When you have the correct PC-DMIS license configured for the HP-C-Ve interface, it ensures the correct files and registry entries are set up when you install PC-DMIS.

The HP-C-Ve interface requires these license options:

- Vision enabled

- CMM-V DCC Vision type

- Leitz/FDC interface enabled

If done correctly, the PC-DMIS installation renames the following files:

- HSI_CMMV.dll to HSI.dll

- Leitz.dll or FDC.dll to InterfacHelper.dll

- HEXMSI.dll to Interfac.dll

The PC-DMIS installation assumes that the FrameGrabber has already been successfully installed. Framegrabber installation details are beyond the scope of this document.