miim

### DCC-3 DCC to MP interrupt not acknowledged for 32 milliseconds

The DCC sent an interrupt to the MP. The MP has not acknowledged the interrupt in the last 32 milliseconds.

For more information, see "DCC Error Codes".

What you should do:

1. To clear the error, power the MP down.

2. Reseat the DCC board.

3. Reseat the MP CPU board.

4. Power the MP back up.

5. If the error reoccurs, contact your Giddings & Lewis service representative.