core

### Location Options

PC-DMIS also allows you to show these specialty axes:

- Retrolinear Only

- Gap Only

- Half Angle

These options can be selected in the Locations Options area in the Feature Location dialog box (Insert | Dimension | Location). All future locations of vector, surface, and edge points within the measurement routine is printed using the appropriate specialty axes until the option is turned OFF.

More:

Retrolinear Only for Location Dimensions

Gap Only for Location Dimensions

Half Angle for Location Dimensions