miim

### MP-094 APC lid timeout error

The APC has reported that a station lid was in the open position for an excessive amount of time.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

2. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

3. If the error reoccurs, contact your Giddings & Lewis service representative.