miim

#### Operator Panel Functions

When you use the jog box or operator panel, CMM-OS generates notification strings.

For example, CMM-OS generates these notification strings and assigns the proper string value to the designated registry entry:

PanelcodeDone = "F1" - CMM-OS generates the notification string "Panelcode-F1". PC-DMIS then assigns "F1" to the PanelcodeDone registry entry. An empty string disables this function.

PanelcodeEraseHit = "F2" - CMM-OS generates the notification string "Panelcode-F2". PC-DMIS then assigns "F2" to the PanelcodeEraseHit registry entry.

PanelcodeStop = "F4" - CMM-OS generates the notification string "Panelcode-F4". PC-DMIS then assigns "F4" to the PanelcodeStop registry entry.

PanelcodeInsertMove = "TWPoint" - CMM-OS generates the notification string "Panelcode-TWPoint". PC-DMIS then assigns "TWPoint" to the PanelcodeInsertMove registry entry. This code is the code sent by a button on the top of the right-hand joystick.