Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
InsertionPointAfter Method
See Also Send Topic Feedback | See Object Hierarchy Chart

Command
  Required Command object that indicates the command after which to set the insertion point.

PCDLRN ActiveX DLL > Commands Object : InsertionPointAfter Method

Glossary Item Box

# Description

Sets the insertion point after a specified command.

# Syntax

Visual Basic
    Public Function InsertionPointAfter( _
       ByVal Command As Command _
    ) As Boolean

# Parameters

Command
  Required Command object that indicates the command after which to set the insertion point.

# Return Type

Boolean value. This function returns TRUE if the insertion point was successfully set, FALSE otherwise.

# Example

For an example, see the example in GetReferencedFeature.

# See Also

Commands Object | Commands Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.