settingseditor

### AlignmentIterateRePierce

This registry entry determines whether or not an iterative best-fit alignment is performed. If enabled, the alignment pierces the CAD geometry and adjusts the feature nominals for each iteration by using the RepierceTolInMM and MaxIterations registry entries to control the result.

Entry Name: AlignmentIterateRePierce

Entry Type: Whole Number. Setting this to 1 tells PC-DMIS to perform an iterative best fit alignment. The default value is 0.