core

#### Gage Scan Filter

(This item pertains to the Edit Probe Data dialog box. You can open this dialog box with the Edit button on the Probe Utilities dialog box, accessible through Insert | Hardware Definition | Probe.)

The Gage Scan Filter box in the Edit Probe Data dialog box displays the type of gage scan filter compensation for the selected probe tip: None, Software, or Hardware.

It also indicates how the gage scan filter was calibrated:

- (In) - with an inside circle

- (Out) - with an outside circle

- (Both) - with both an inside circle and an outside circle

For more information about the gage scan filter, see the "Enabling the Gage Scan Filter" topic in the "PC-DMIS CMM" documentation.