core

#### Form Only

When dimensioning a profile, selecting the Form Only option in the Surface Profile dialog box (Insert | Dimension | Profile | Surface), you can tell PC-DMIS to only determine if a particular profile matches the same form as its nominal. This option ignores whether the location of the profile is outside of acceptable tolerances.

For a Form Only dimension, pay attention to the measured values in the generated dimension.