core

### Constructing an Offset Point

You can construct a point a specified distance from any input feature.

To construct an offset point:

1. Access the Construct Point dialog box (Insert | Feature | Constructed | Point).

2. Select the Offset Point option from the list of options.

3. Select a feature from which to create the offset point.

4. Click the Create button.

To create an offset point from the origin, select the At Origin option. To create an offset point relative to a particular feature, select the desired feature and type the values in the X offset, Y offset, and Z offset boxes.