miim

#### Frame Grabber

For additional details, refer to factory setup documentation.

To install the software and configure the frame grabber hardware:

1. Install the frame grabber software.

2. Install the board in the PC.

3. Reboot the PC.

4. Verify the device is working properly in the device manager.

5. Run PC-DMIS in administrator mode.

6. Close PC-DMIS.

7. Configure the PC-DMIS frame grabber / camera settings. For more details, see the topics "Settings" and "Latching".

8. Run PC-DMIS. Confirm the live image view is working.