settingseditor

### 5UniqueGripperOffset(XYZ)

This registry entry is not used.

The three values store the values of the gripper offsets after calibration or your 5 Unique fixturing system. The gripper offset is treated the same as a probe offset. The center of the gripper is hereby linked to the machine.

Entry Name: 5UniqueGripperOffset(XYZ)

Entry Type: Real Number values that define the gripper offset. These are the default values:

For X and Y

0

For Z

149