core

## PC-DMIS Offline Prerequisites

To use PC-DMIS in Offline mode, CAD data in the form of an IGES model, a DES file, a DXF file, or X,Y,Z,I,J,K data must be available. The "Importing CAD Data or Feature Data" topic in the "Using Advanced File Options" chapter has information on how to import these files into the PC-DMIS system.

More:

IGES Entities Supported

DXF Input

DES Input

XYZ ASCII File