cmm

#### Path Definition Tab - Adaptive Circle Scan Strategy

The Path Definition tab for the Adaptive Circle Scan strategy provides you with additional options to define a circular scan path. You can view the scan path whenever you update a path definition parameter. You can also view the updated scan path in the Graphic Display window.

Control Element

Select whether the circle scan will be done on a cylindrical shape or a spherical shape.

Path Density

Type the number of points per mm that will be generated to create the scan path.

Sphere Center

This property appears when you select Spherical in the Control Element list. For this property, the vectors of the derived scan are not in the plane of the circle, but are normal to the sphere surface. One use for this scan type is the ISO 10360-4 tests. The X, Y, and Z boxes are the part coordinates.