qdasconfigurator

### Supported K-Fields

Q-DAS Configurator supports the list of K-fields in the following table:

Key | Type | Length | Field Name
K0001 | F | 22 | Measured Value
K0002 | I5 | 5 | Attribute
K0004 | D | --- | Time
K0005 | S | --- | Event
K0006 | AN | 14 | Batch Number
K0007 | I10 | 10 | Cavity Number
K0008 | I10 | 10 | Operator Name
K0009 | AN | 255 | Text
K0010 | I10 | 10 | Machine Number
K0011 | S | --- | Process Parameter
K0012 | I10 | 10 | Gage Number
K0013 | I5 | 5 | Process Parameter Value
K0014 | AN | 40 | Part ID Number
K0015 | I5 | 5 | Reason for Test
K0016 | AN | 30 | Production Number
K0017 | AN | 30 | Workpiece Fixture Number
K0020 | I5 | 5 | Subgroup Size
K0021 | I5 | 5 | Number of Errors
K0053 | AN | 20 | Order
K0054 | AN | 30 | K0054
K0055 | AN | 30 | K0055
K0056 | AN | 30 | K0056
K0057 | AN | 30 | K0057
K0058 | AN | 30 | K0058
K0059 | AN | 30 | K0059
K0060 | AN | 30 | K0060
K0061 | I10 | 10 | K0061
K0062 | I10 | 10 | K0062
K0063 | I10 | 10 | K0063
K0080 | AN | 64 | Subgroup ID
K0081 | I5 | 5 | Value Position in Subgroup
K0100 | I5 | 5 | Total Number of Characteristics in File
K1001 | AN | 30 | Part Number
K1002 | AN | 80 | Part Description
K1003 | AN | 20 | Part Abbreviation
K1004 | AN | 20 | Part Amendment Status
K1005 | AN | 40 | Product
K1007 | AN | 20 | Abbreviation Part Number
K1008 | AN | 20 | Part Type
K1009 | AN | 20 | Part Code
K1010 | I3 | 3 | Control Item
K1011 | AN | 20 | Version
K1014 | AN | 20 | Part Identification
K1021 | AN | 20 | Manufacturer Number Text
K1022 | AN | 80 | Manufacturer Name
K1031 | AN | 20 | Material Number Text
K1032 | AN | 80 | Material Description
K1041 | AN | 30 | Drawing Number
K1042 | AN | 20 | Drawing Amendment
K1043 | AN | 80 | Drawing Index
K1052 | AN | 80 | Contractor Description
K1053 | AN | 40 | Contract
K1061 | AN | 20 | Customer Number Text
K1062 | AN | 40 | Customer Description
K1071 | AN | 20 | Supplier Number Text
K1072 | AN | 40 | Supplier Name
K1081 | AN | 24 | Machine Number
K1082 | AN | 40 | Machine Description
K1083 | I5 | 5 | Machine Number
K1085 | AN | 40 | Machine Location
K1086 | AN | 40 | Work Cycle / Operation Number
K1087 | AN | 40 | Production Cycle Description
K1100 | AN | 40 | Plant Sector
K1101 | AN | 40 | Department
K1102 | AN | 40 | Workshop / Sector
K1103 | AN | 40 | Cost Center
K1104 | AN | 20 | Shift
K1110 | AN | 20 | Order Number
K1111 | AN | 20 | Goods Received Number
K1201 | AN | 24 | Test Facility Number
K1202 | AN | 40 | Test Facility Description
K1203 | AN | 80 | Reason for Test
K1206 | AN | 40 | Test Location
K1209 | AN | 20 | Inspection Type
K1210 | I5 | 5 | Measurement Type
K1221 | AN | 20 | Inspector Number (Text)
K1222 | AN | 40 | Inspector Name
K1230 | AN | 40 | Gage Room
K1231 | AN | 20 | Measuring Program Number
K1232 | AN | 20 | Measuring Program Version
K1302 | AN | 40 | Test Batch
K1303 | AN | 40 | Plant
K1311 | AN | 40 | Production Order
K1341 | AN | 20 | Test Plan Number Text
K1343 | D | 20 | Test Plan Development Date
K1344 | AN | 40 | Test Plan Developer
K1802 | AN | 255 | User Field Content 1
K1812 | AN | 255 | User Field Content 2
K1822 | AN | 255 | User Field Content 3
K1832 | AN | 255 | User Field Content 4
K1842 | AN | 255 | User Field Content 5
K1852 | AN | 255 | User Field Content 6
K1860 | AN | 50 | User Field Description 7
K1861 | AN | 1 | User Field Type 7
K1862 | AN | 255 | User Field Content 7
K1900 | AN | 255 | Remark
K1997 | AN | --- | Parts GUID
K2001 | AN | 20 | Characteristic Number
K2002 | AN | 80 | Characteristic Description
K2003 | AN | 20 | Characteristic Abbreviation
K2004 | I5 | 5 | Characteristic Type
K2005 | I5 | 5 | Characteristics Class
K2006 | I5 | 5 | Control Item
K2007 | I5 | 5 | Control Type
K2008 | I5 | 5 | Group Type
K2009 | I5 | 5 | Measured Quantity
K2015 | I3 | 3 | Tool Wear Type
K2016 | I3 | 3 | 100% Measurement
K2022 | I5 | 5 | Decimal Places
K2030 | I5 | 5 | Group Number
K2031 | I5 | 5 | Group Element Number
K2043 | AN | 40 | Recording Device Name
K2060 | I5 | 5 | Events Catalog
K2061 | I5 | 5 | Process Parameter Catalog
K2062 | I5 | 5 | Cavity Catalog
K2063 | I5 | 5 | Machine Catalog
K2064 | I5 | 5 | Gage Catalog
K2065 | I5 | 5 | Operator Catalog
K2066 | I5 | 5 | Subcatalog K0061
K2067 | I5 | 5 | Subcatalog K0062
K2068 | I5 | 5 | Subcatalog K0063
K2092 | AN | 50 | Characteristic Text
K2093 | AN | 80 | Processing Status
K2095 | AN | 40 | Element Code
K2096 | AN | 20 | Element Index
K2097 | AN | 50 | Element Text
K2100 | F | 22 | Target Value
K2101 | F | 22 | Nominal Value
K2110 | F | 22 | Lower Specification Limit
K2111 | F | 22 | Upper Specification Limit
K2112 | F | 22 | Lower Allowance
K2113 | F | 22 | Upper Allowance
K2114 | F | 22 | Lower Scrap Limit
K2115 | F | 22 | Upper Scrap Limit
K2120 | I3 | 3 | Lower Limit Value
K2121 | I3 | 3 | Upper Limit Value
K2130 | F | 22 | Lower Plausibility Limit
K2131 | F | 22 | Upper Plausibility Limit
K2142 | AN | 20 | Unit
K2202 | I3 | 3 | Evaluation Type
K2203 | I3 | 3 | Car Body Mode
K2205 | I5 | 5 | Number of Parts
K2211 | AN | 40 | Master Number
K2212 | AN | 40 | Master Description
K2213 | F | 22 | Standard Actual Value
K2216 | AN | 20 | Master - Serial Number
K2220 | I5 | 5 | Number of Operators
K2221 | I5 | 5 | Number of Trials
K2222 | I5 | 5 | Number of Reference Measurements
K2281 | AN | 40 | Calibrating Part - Center Number
K2301 | AN | 20 | Machine Number
K2302 | AN | 40 | Machine Description
K2303 | AN | 40 | Department / Cost center
K2311 | AN | 20 | Production Type
K2312 | AN | 40 | Production Type Description
K2320 | AN | 20 | Contract Number
K2401 | AN | 40 | Gage Number
K2402 | AN | 80 | Gage Description
K2403 | AN | 20 | Gage Group
K2404 | F | 22 | Gage Resolution
K2406 | AN | 40 | Gage Manufacturer
K2407 | AN | 20 | SPC Device Number
K2408 | AN | 20 | SPC Device Manufacturer
K2409 | AN | 20 | SPC Device Type
K2410 | AN | 40 | Test Location
K2411 | D | 40 | Test Begin
K2415 | AN | 20 | Gage Serial Number
K2434 | I5 | 5 | Proof of Process Capability
K2440 | AN | 40 | Assembly Component
K2505 | AN | 20 | View Description
K2506 | I3 | 3 | Sheet Number
K2630 | F | 22 | Calibration Uncertainty
K2802 | AN | 255 | Tool Number / Tool Name
K2810 | AN | 50 | Lower Reaction Limit
K2812 | AN | 255 | Experience Value
K2820 | AN | 50 | Upper Reaction Limit
K2822 | AN | 255 | Floating Average Factor
K2830 | AN | 50 | Compensation on Reject
K2832 | AN | 255 | No Correction Range
K2840 | AN | 50 | Calculation Direction
K2842 | AN | 255 | Maximum Compensation
K2850 | AN | 50 | Tool Geometry
K2852 | AN | 255 | Reference Geometry
K2860 | AN | 50 | Tool Compensation
K2862 | AN | 255 | Action in Case of Tool Violation
K2870 | AN | 50 | Tool Wear Limit
K2872 | AN | 255 | Alpha Compensation
K2880 | AN | 50 | Spindle / Head Number / Name
K2882 | AN | 255 | Roughing Tool Number / Name
K2890 | AN | 50 | Add Value for Rougher
K2892 | AN | 255 | Part Skip Value
K2900 | AN | 255 | Remark
K2991 | AN | 255 | PCD ID
K5001 | AN | 30 | Group Number (Text)
K5002 | AN | 80 | Group Description
K5101 | I5 | 5 | Part as Part of a Group
K5102 | I5 | 5 | Characteristic as Part of a Group
K5103 | I5 | 5 | Group as Part of a Group
K5111 | I5 | 5 | Parts Group
K5112 | I5 | 5 | Characteristics Group
K5113 | I5 | 5 | Group Element
K8010 | S | --- | Chart Type (Location)
K8011 | F | 22 | Central Position (Location)
K8012 | F | 22 | Lower Control Limit (Location)
K8013 | F | 22 | Upper Control Limit (Location)
K8014 | F | 22 | Lower Warning Limit (Location)
K8015 | F | 22 | Upper Warning Limit (Location)
K8110 | S | --- | Chart Type (Variation)
K8111 | F | 22 | Central Position (Variation)
K8112 | F | 22 | Lower Control Limit (Variation)
K8113 | F | 22 | Upper Control Limit (Variation)
K8114 | F | 22 | Lower Warning Limit (Variation)
K8115 | F | 22 | Upper Warning Limit (Variation)
K8500 | I5 | 5 | Subgroup Size
K8501 | I3 | 3 | Subgroup Type
K8502 | AN | 40 | Subgroup Frequency
K8503 | I3 | 3 | Stable Subgroup Size
K8504 | I5 | 5 | Subgroup Incidence
K8505 | I5 | 5 | Number of Parts (ELS)
K8520 | F | 22 | Required Cp Value
K8521 | F | 22 | Required Cpk Value
K8522 | F | 22 | Fixed Cp Value
K8523 | F | 22 | Fixed Cpk Value
K8600 | I3 | 3 | Correction Strategy
K8610 | F | 22 | Lower Correction Limit
K8611 | F | 22 | Upper Correction Limit
K8612 | I3 | 3 | Buffer Size
K8613 | F | 22 | Correction Target Value