cmm

#### Advanced Tab - Adaptive Cylinder Spiral Scan Strategy

Use the Advanced tab for the Adaptive Cylinder Spiral Scan strategy to override the calculated settings and any automatically configured parameters.

Override

If you select this check box, it overrides any automatically configured parameters. It also enables the Point Density, Scan Speed, Acceleration, and Offset Force properties, which you can use to change the scanning characteristics for this measurement.

Point Density

Type or select the number of readings to take per unit of measurement during the scan.

Scan Speed

Type or select the scan speed (mm/sec).

Acceleration

Type or select the acceleration to use during a scan. The value is specified in mm/sec/sec.

Offset Force

Type or select the level of force to maintain during a scan. The value is specified in newtons.

Scan Type

Select the type of scan that you want to execute on the controller:

- Defined - Executes the defined path scan on a B3C, B4, or FDC controller.

- CIR - Executes the CIR type of scan on a B4 or B5 Leitz controller.