core

### To Dimension a Feature Using the CYLINDRICITY Option

1. Select Insert | Dimension | Cylindricity from the submenu. The Cylindricity dialog box will appear.

2. Select the feature(s) to dimension from the Feature List box. You can only select cylinder features.

3. Type the plus tolerance value in the Plus box.

4. Select either Inch or MM in the Units section.

5. Select where to output the dimension information. Select the Statistics, Report, Both, or None option.

6. Select the optional Display check box if you want to view dimension information in the Graphic Display window.

7. Select the desired Analysis options by marking the Textual check box or the Graphical check box. If the Graphical check box was marked, enter the Multiplier value in the Multiplier box.

8. If desired, select the Display check box in the Dimension Info area and click Edit to select the Dimension Info Format you would like displayed in the Graphic Display window.

9. Click the Create button.

The dimension will appear in the Edit window with this information:

dimension_name = CYLINDRICITY,OF feat_1

AX | NOM | +TOL | -TOL | MEAS | MAX | MIN | DEV | OUT-TOL
M | 0.0000 | 0.0100 | 0.0100 | 5.0000 | 0.0000 | 0.0000 | 0.0000 | 0.0000