Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
LEAPFROG Object Members
See Also Overview Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL : LEAPFROG Object

Glossary Item Box

# Public Properties

full | Determines whether or not the leapfrog will be full (1) or partial (0). For more information on this, see the "Creating and Using Alignments" topic in the PC-DMIS Help File.
leapfrogtype | Integer value that defines the type of feature used to translate the CMM along the part.
NumHits | Integer value that determines the number of hits used for the feature types described in the LeapFrogType property. The feature type determines if the number of hits are useful or not.

# See Also

LEAPFROG Object

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.