miim

### LK Direct TCP Interface Updates

Version | Description
1.11 | Modified decryption method to support x64 (PCD-104300). Added support for the new LK jog box (PCD-104301).
1.10 | Fixed issue when relative speed was too small, touch mode fails in Jog Box Fast mode (PCD-25627).
1.09 | Added additional check for machine move start. Corrected circular move response for machines that send multiple responses for one fly move. Added support for Fly Mode. Fixed problem where Auto-Slot was taking double hits.
1.08 | Fixed issue where VNass-Numerous was hanging (PR# 273888). Added checks for Superfluous 'G' when responses arrived together. Removed response requirement for Manual Hit Clear.
1.07 | Final fix for Bosch circular moves. Tested on site at Draexlmaier (PR# 273745).
1.06 | Fixed bug that missed response when two responses were returned together. Fixed bug with relative moves that did not consider retracts position (PR# 272635). Fixed bug occurring with large circular moves (PR# 272245).
1.05 | Fixed for hit vector not recognized due to non-conversion from inches (PR# 272669).
1.04 | Fixed for "Probe not Armed" error after tool change.
1.03 | Corrected long delay at start of execution due to queued goManual commands. Corrected speed calculation.
1.02 | Added flag for support of controllers requiring only a single response for circular moves.
1.01 | Added support for MCC-200 (TPC) controller. Fixed problem with Find Hole. Corrected DCC retract use of wrong param ID.
1.0 | Improved error handling. Added option to disable "Print" as END key from jog box.
0.90n | Initial release for IP-based LK scanning CMMs.