core

## Setting Probe Depth

To program measurements in Offline mode, it is important to set the depth of the probe at a specified distance (in relation to the surface of the current workplane). PC-DMIS offers several methods to set the probe’s depth.

PC-DMIS must be in Program mode to use any of these techniques.

More:

Setting Approximate Probe Depth

Setting Probe Depth on a Feature

Setting Probe Depth on a Sphere

Setting Probe Depth on a Cone

Keying in Probe Depth