core

### Regenerating the Path

The Operation | Graphic Display Window | Regenerate Path menu option erases the current path lines and re-draws them.

You may want to regenerate your path when you've made changes to a measurement routine, and you want your path lines to reflect the current state of the measurement routine.

Notes:

- Regenerate Path is only accessible after you mark features in the Edit window and you select the View | Path Lines option.

The software only generates the probe's path lines for features that follow a MODE/DCC command. If your measurement routine doesn't have a MODE/DCC command, you won't see any path lines.

- Regenerate Path is not available for Portable devices.

- You can press Esc to cancel the regeneration at any time.

- If you insert a move before a PH9 wrist change, the location of the wrist change does not move until you choose Regenerate Path.