core

#### Touch Speed

TOUCHSPEED/nnn.nnnn

nnn.nnnn represents a number value for the speed. This command changes the speed at which the CMM takes hits. Depending on the state of the Display absolute speeds check box in the Part/Machine tab of the Setup Options dialog box (Edit | Preferences | Setup), this is either an absolute speed (mm/sec) or a percentage of the machine's total speed capability.