miim

### MP-047 Temperature Compensation D/A failure

A D/A conversion on the Temperature Compensation board failed to complete within the allotted time of 32 milliseconds.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, contact your Giddings & Lewis service representative.