portable

#### B-Probe Button Assignments

B-Probe Buttons

Button 1 - Button 1 functions are:

- Click and hold to turn on.

- Once the probe turns on, use the button to take measurements.

Button 2 - Button 2 functions are:

- Click and hold to turn on.

- Once the probe turns on, use the button to take measurements.

- Click and hold to turn the probe off.

IJK Behavior on B-Probe Points

If aligned to the part, PC-DMIS always stores IJK values perpendicular to one of the active coordinate system axes, except if you use Point Only mode.