fixturing

#### List of Global Settings for Manual Machines

- FixtureLocation - The path where you want the fixture files (.ext. and .fxt ) to be saved.

- ModuleLocation - The full path of the location where modules are saved.

- StatusLocation - The location where the fixture data file is saved.

- Standby Values for automatic standby:

- Create Standby Command(0/1)

- Optional Settings

- Standby Plane - Set this to XY for vertical and ZX for robots

- Common Axis convention - 0 = Convention for Horizontal CMM (default); 1 = Global with common axis