settingseditor

## AutoInsertMoves

The registry entries in this section are used with the PC-DMIS capability to automatically insert clearance moves within PC-DMIS Inspection Planner. These are used in the Auto Create Clearance Moves dialog box.

The following registry entries provide the criteria for how clearance moves are added to your imported Inspection Plan:

More:

BelowTriggerTolerancePercentage

ClearanceCubeOffsetMM

CollisionMoveClearanceInMM

CollisionToleranceInMM

ConeAngleForMoveOverPath

DeleteMovesBeforeInsert

MaximumAttempts

OMPLAutoInsertMoves

SolutionTime_OMPL

MaximumSolutionTime_OMPL

SmallestTipSearchIncrementInDegrees