core

#### Hard Probe Scanning Minimums Area

The Hard Probe Scanning Minimums area is disabled for trackers that do not support this functionality.

Time Delta (sec) box

This value allows PC-DMIS to reduce the amount of points that are scanned by deleting hits that are read in faster than the specified time delay in milliseconds.

Distance Delta box

This value allows you to reduce the measured data by deleting hits that are closer than the distance specified in millimeters. The reduction of hits happens as data comes from the machine. PC-DMIS only keeps the points that are set apart by more than the specified increments.