Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
CreateRoutineFromInspectionPlan Method
See Also Send Topic Feedback | See Object Hierarchy Chart

FileName

  This is the file name to give the created measurement routine.

  - If this is an empty string, PC-DMIS displays a dialog so you can type in the name of the routine.
  - If this is a full path, the routine is created at that location.
  - If this is just a string for a file name, the routine is created in the default folder PC-DMIS uses for measurement routines.

CadFileName

  Required String. This is the file name to use for the CAD file used by the measurement routine. This needs to be a full pathway file name to the CAD file. The extension can be any CAD file extension that PC-DMIS can import (such as .cad, .igs, .dxf, and so on).

PlanFileName
  Required String. This is the file name of the inspection plan that the measurement routine is created from. This needs to be a full pathway file name to the inspection plan (.xml or.planxml).

MachineName

  Required String. This is the identifying string for your machine. If you're running in offline mode, use "Offline". If you're running in online mode use "CMM1".

PCDLRN ActiveX DLL > PartPrograms Object : CreateRoutineFromInspectionPlan Method

Glossary Item Box

# Description

Creates a measurement routine from an inspection plan and then adds the routine as part of a PartPrograms collection.

# Syntax

Visual Basic
    Public Function CreateRoutineFromInspectionPlan( _
       ByVal FileName As String, _
       ByVal CadFileName As String, _
       ByVal PlanFileName As String, _
       ByVal MachineName As String _
    ) As PartProgram

# Parameters

FileName

  This is the file name to give the created measurement routine.

  - If this is an empty string, PC-DMIS displays a dialog so you can type in the name of the routine.
  - If this is a full path, the routine is created at that location.
  - If this is just a string for a file name, the routine is created in the default folder PC-DMIS uses for measurement routines.
CadFileName

  Required String. This is the file name to use for the CAD file used by the measurement routine. This needs to be a full pathway file name to the CAD file. The extension can be any CAD file extension that PC-DMIS can import (such as .cad, .igs, .dxf, and so on).

PlanFileName
  Required String. This is the file name of the inspection plan that the measurement routine is created from. This needs to be a full pathway file name to the inspection plan (.xml or.planxml).
MachineName

  Required String. This is the identifying string for your machine. If you're running in offline mode, use "Offline". If you're running in online mode use "CMM1".

# Return Type

PartProgram object.

# Remarks

This method only runs properly if the Application.MMSInspectConnected method returns True.

# See Also

PartPrograms Object | PartPrograms Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.