settingseditor

### CW43LTThirdAxisSlotAngle

Use this registry entry to tell PC-DMIS the third axis angle position of the probe inside the tool changer slot.

This registry entry appears in the LEITZ section of the Settings Editor when the PC-DMIS interface is LEITZ. It appears in the FirmwareDistributedController(FDC) section of the Settings Editor when the PC-DMIS interface is FDC.

Entry Name: CW43LTThirdAxisSlotAngle

Entry Type: Whole number. Set the third axis angle position inside the tool changer slot. If the value is -1, the angle value is the default value (according to the slot type). You can set a value in these ranges:

- 0 to 180

- 0 to -180