Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
DoAutoInsertMoves Method
See Also Example Send Topic Feedback | See Object Hierarchy Chart

StartCommand

endCommand

PCDLRN ActiveX DLL > PartProgram Object : DoAutoInsertMoves Method

Glossary Item Box

# Description

This method can take two parameters, a start command and an end command. These define a range of commands. The method then adds MOVE/POINT commands between each feature command within this range. If you don't specify a start or end command then the range includes all the features in the measurement routine.

# Syntax

Visual Basic
    Public Function DoAutoInsertMoves( _
       ByVal StartCommand As Command, _
       ByVal endCommand As Command _
    ) As Boolean

# Parameters

StartCommand
endCommand

# Return Type

This returns True if the moves were added. This returns False if they weren't.

# Example

Example (VBScript) | Copy Code
--- | ---
    Dim DmisApp As Object
    Dim DmisPart As Object

    Sub Main
      Set DmisApp = CreateObject("PCDLRN.Application")
      Set DmisPart = DmisApp.ActivePartProgram

      DmisPart.DoAutoInsertMoves Nothing, Nothing

    Set DmisPart = Nothing
    Set DmisApp = Nothing

    End Sub

# See Also

PartProgram Object | PartProgram Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.