Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
BoundaryCondition Property
See Also Send Topic Feedback | See Object Hierarchy Chart

PCDLRN ActiveX DLL > BasicScan Object : BoundaryCondition Property

Glossary Item Box

# Description

Represents the boundary condition type.

# Syntax

Visual Basic
    Public Property BoundaryCondition As BSBOUNDCOND_ENUM

# Return Type

Read/write of enumeration BSBOUNDCOND_ENUM.

# Remarks

The allowable values are:

BSBOUNDCOND_SPHERE

BSBOUNDCOND_PLANECROSS

BSBOUNDCOND_CYLINDER

BSBOUNDCOND_CONE

The SetBoundaryConditionParams method should be used to set the values for:

- HalfAngle
- Number of Crossings
- Diameter

# See Also

BasicScan Object | BasicScan Members | SetBoundaryConditionParams Method | SetBoundaryConditionParams Method

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.