dci

##### Create a New Measurement Routine

1. Select File | New to open the New Measurement Routine dialog box.

2. In the Part Name box, type a name for the measurement routine, and fill in the other boxes if desired.

3. From the Measurement Units area, select the units of measurement. This should match the units used in the CAD file you will import.

4. Click OK. This dialog box closes and the Probe Utilities dialog box opens.

5. To close the Probe Utilities dialog box, click Cancel.

6. Click OK.

Calibrate the probe if you wish. If you choose to not calibrate the probe, PC-DMIS displays a message stating that the probe has not been calibrated. Click OK to continue.