miim

### MP-183 Probe changer rack disconnected

The probe changer control unit and the probe changer rack are not connected to one another.

What you should do:

1. Connect the probe changer control unit to the probe changer rack.

2. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

3. If the error reoccurs, contact your Giddings & Lewis service representative.