Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
GetPoint Method
See Also Send Topic Feedback | See Object Hierarchy Chart

PointType
  FPOINT_TYPES enumeration.

TheoMeas
  Enumerated Long value.

X
  Variable of type double that will hold the X data for the point.

Y
  Variable of type double that will hold the Y data for the point.

Z
  Variable of type double that will hold the Z data for the point.

PCDLRN ActiveX DLL > FeatCmd Object : GetPoint Method

Glossary Item Box

# Description

This method retrieves point information for individual objects.

# Syntax

Visual Basic
    Public Function GetPoint( _
       ByVal PointType As FPOINT_TYPES, _
       ByVal TheoMeas As FDATA_DATASET, _
       ByRef X As Double, _
       ByRef Y As Double, _
       ByRef Z As Double _
    ) As Boolean

# Parameters

PointType

  Value | Description
  --- | ---
  FPOINT_BALLCENTER |
  FPOINT_CENTROID |
  FPOINT_ENDPOINT |
  FPOINT_MIDPOINT |
  FPOINT_SNAP_CENTROID |
  FPOINT_STARTPOINT |

  FPOINT_TYPES enumeration.
TheoMeas

  Value | Description
  --- | ---
  FDATA_ALL |
  FDATA_MEAS |
  FDATA_TARG |
  FDATA_THEO |

  Enumerated Long value.
X
  Variable of type double that will hold the X data for the point.
Y
  Variable of type double that will hold the Y data for the point.
Z
  Variable of type double that will hold the Z data for the point.

# Return Type

Boolean value indicating success or failure of the call.

# See Also

FeatCmd Object | FeatCmd Members | PutPoint Method

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.