planner

## The Insert Menu

Insert | Feature | Constructed | <Feature> - Uses a construction dialog box to create the feature from existing features.

Insert | Feature | Generic - Creates a generic feature. Generic features are often used to control the measured and theoretical values of a specific feature in order to perform calculations that constructed features don't currently support.

Insert | Alignment | New - Displays the Alignment Utilities dialog box so you can create an alignment that aligns your part to the coordinate system.

Insert | Alignment | Save - Saves a modified alignment.

Insert | Alignment | Equate - Equates a new alignment with an original alignment.

Insert | Dimension | Datum Definition - Defines existing features as datums.

Insert | Dimension | <Type> - Opens a dialog box so you can select the feature or features to dimension and insert the dimension into the inspection plan. For dimension types that support Feature Control Frames (FCF), the XactMeasure GD&T dialog box opens so you can insert the dimension as a FCF.

Insert | Dimension | Keyin - Displays the Dimensional Keyin dialog box so you can define a dimension entirely through the keyboard, as opposed to dimensioning around a created feature.

Insert | Report Command | Comment - Inserts a comment into the inspection plan. For information on comments, see "Inserting Programmer Comments".