miim

### MP-092 APC GO message timeout

The APC reported that the probe changer screw failed to turn within the allowed time.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, contact your Giddings & Lewis service representative.