settingseditor

### AutoShutterTimeToFire

When PC-DMIS detects that the Region of Interest (ROI) is ready to fire, this registry entry provides a delay (in milliseconds) that PC-DMIS waits before issuing the point detect command. This delay gives the stage a chance to settle before firing the point detection. This value is only evaluated for the first ROI. Subsequent ROIs are evaluated with the value for the AutoShutterTimeToFireNth registry entry.

This registry entry is only evaluated when the AutoShutterEnable registry entry is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

This value relates to the Movement Feature settle in the Live View Setup dialog box. For information, see the "Setting up the Live View" topic in the PC-DMIS Vision documentation.

Entry Name: AutoShutterTimeToFire

Entry Type: Whole Number to specify milliseconds. The default value is 3000.