portable

#### Contour.dll Registration

To manually register the Contour.dll file, follow these steps:

1. Check that the power on the Perceptron Sensor controller box is on as well as the power to the arm.

2. Open a Command Prompt window (DOS prompt), and change to the Perceptron directory. This is a subdirectory of the main PC-DMIS install directory.

3. Type the following on the command line: "regsvr32 contour.dll". After a few seconds, you should get a message that says "Contour.dll registered successfully".

4. If the file does not register successfully, contact Hexagon Technical Support. Otherwise, restart PC-DMIS.