settingseditor

### Cylinder_CGGraySumMaterial

This registry entry specifies the material type that is used when measuring laser cylinder features. The associated minimum and maximum pixel intensity are used. If this registry entry is set to -1, then the custom values specified with the Cylinder_CGGraySumMax and Cylinder_CGGraySumMin registry entries are used.

Entry Name: Cylinder_CGGraySumMaterial

Entry Type: Whole number that specifies the feature material type. The default value is -1 (Custom).

Value | Material Type
-1 | Custom
0 | Sheet Metal
1 | White
2 | Blue
3 | Black
4 | Aluminum
5 | Ceramic
6 | Tungsten