core

### POINTINFO Command

The POINTINFO command is created by the Edit Point Info dialog box (Insert | Report Command | Edit Point info).

When a POINTINFO command has been inserted in the measurement routine, a Point Info box is displayed in the Graphic Display window. The POINTINFO command can be modified in the Edit window. The command line for the POINTINFO command reads:

POINTINFO/Dim ID or Feat ID; FILTER FILTER_TYPE FILTER_NUM;ICON,ID,TYPE,VERT,HORIZ; HEADINGS, GRAPH; ”OUTPUT FORMAT” ,$
"HIT NUMBERS"

Dim ID or Feat ID - The ID of the dimension or feature to be displayed.

FILTER_TYPE - A toggle string that shows the filter option of NONE, INTERVAL, WORST, DEVIATION, or OUTTOL.

FILTER_NUM - A number field available when the filter option is INTERVAL, WORST, or DEVIATION.

ICON - A toggle string that shows a blank when it is OFF, and "ICON" when it is ON. When it is ON, the POINTINFO will display the dimension or feature ID with the appropriate icon.

ID - A toggle string that shows a blank when it is OFF, and "ID" when it is ON. When it is ON, the POINTINFO will display the dimension or feature ID with the point information.

TYPE - A toggle string that shows a blank when it is OFF, and "TYPE" when it is ON. When it is ON, the POINTINFO will display feature or dimension type (i.e. CIRCLE, POINT, ROUNDNESS, LOCATION) with the point information.

VERT - A toggle string that shows a blank when it is OFF, and "VERT" when it is ON. When it is ON, the POINTINFO will display with the vertical lines between the columns.

HORIZ - A toggle string that shows a blank when it is OFF, and "HORIZ" when it is ON. When it is ON, the POINTINFO will display with the horizontal lines between the rows.

HEADINGS - A toggle string that shows a blank when it is OFF and "HEADINGS" when it is ON. When it is ON, the row headers will be displayed in the Point Info box.

GRAPH - A toggle string that shows a blank when it is OFF and "GRAPH" when it is ON. When it is ON, the dimension percentage will be graphically displayed in the Point Info box.

OUTPUT FORMAT - The format of the point information that will be displayed based on the order of selection. Available output options are HIT, PT, V, and DEV. Options cannot be duplicated.

HIT NUMBERS - The hit numbers are the specific numbered hits that are controlled by this particular POINTINFO command. Multiple hits can be displayed using the same POINTINFO command. Each field in the hit numbers is a toggle string. When a hit is ON, the string in the number position is the hit number (1,2,3, etc.). When a hit is OFF, the toggle string displays a blank.