planner

### Constructing a Projected Cylinder

You can construct a cylinder from any feature and a plane. The diameter of the projected cylinder is the diameter of the first input feature (if circular) or twice the probe diameter if not a circular feature. You need to input the length and diameter for bound measurements. If there is only one input feature, the projection is to the workplane.

To construct a Projected Cylinder:

1. Access the Construct Cylinder dialog box (Insert | Feature | Constructed | Cylinder).

2. Select the Projection option.

3. Select either one or two features. If one feature is selected, the feature can be of any type. If two features are selected, the first feature can be of any type. The second feature must be a plane.

4. Click the Create button.