laser

#### Sphere Command Mode Text

The Sphere command inside the Edit window’s Command Mode looks like this:

SPH1 =FEAT/LASER/SPHERE,CARTESIAN,IN,LEAST_SQR

THEO/<1.895,1.91,1>,<0,0,1>,1.895

ACTL/<1.895,1.91,1>,<0,0,1>,1.895

TARG/<1.895,1.91,1>,<0,0,1>

START ANGLE 1=0,END ANG 1=0

START ANGLE 2=0,END ANG 2=0

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,0

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE