Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
GetOrigin Method
See Also Send Topic Feedback | See Object Hierarchy Chart

X
  Required Long variable that receives the X value of the temperature compensation origin.

Y
  Required Long variable that receives the Y value of the temperature compensation origin.

Z
  Required Long variable that receives the Z value of the temperature compensation origin.

PCDLRN ActiveX DLL > TempComp Object : GetOrigin Method

Glossary Item Box

# Description

Gets the reference origin

# Syntax

Visual Basic
    Public Function GetOrigin( _
       ByRef X As Double, _
       ByRef Y As Double, _
       ByRef Z As Double _
    ) As Boolean

# Parameters

X
  Required Long variable that receives the X value of the temperature compensation origin.
Y
  Required Long variable that receives the Y value of the temperature compensation origin.
Z
  Required Long variable that receives the Z value of the temperature compensation origin.

# Return Type

Boolean value.

# See Also

TempComp Object | TempComp Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.