settingseditor

### DccSurfInitHits

Specifies the default Initial Hits value that will be used in the creation of Surface Points. Initial hits are used to measure the plane around the nominal point location for the Surface Point feature. Initial sample hits are taken only on the initial measurement of the feature during execution of the measurement routine.

Entry Name: DccSurfInitHits

Entry Type: Whole Number to specify the number of initial hits. The default value is 3.