nc

## Using PC-DMIS on a Siemens Lathe

This document is intended to describe the use of PC-DMIS on a Siemens NEF400 lathe.

The PC-DMIS lathe macros additionally compute suitable spindle speed to effectively use the spindle as a C axis.

The following topics are described:

- Calibration

- Measurement

- Update Work Offset for a Siemens Lathe

- Update Tool Offset for a Siemens Lathe

- Macros

- Siemens Lathe - NC Gateway Server Configuration

- Running Multiple Versions of PC-DMIS NC

- Conclusion