miim

### MP-059 Renishaw emergency stop error

The Renishaw PI7, PI12, or PI200 probe controller is turned off, an SCR200 over-travel error has occurred or the Renishaw hardware has requested an emergency stop.

What you should do:

1. To clear the error, click Clear error in the XYZ Display window.

To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, contact your Giddings & Lewis service representative.