core

### Filters

(This item applies to the Edit Point Info dialog box, accessible through Insert | Report Command | Point Info).

Filters area

The Filters area allows you to set filter options to be used when displaying individual point information.

None Used - This tells PC-DMIS not to use any filtering for the POINTINFO command. All hits selected will be displayed with the POINTINFO command.

Hit Interval - This checks the integer value in the box to its right, and only displays the particular hit interval chosen with the POINTINFO command. For example, if 2 were chosen, then every 2nd hit would be displayed, if 3, then every 3rd hit, if 4 then every 4th hit, etc.

Worst - This checks the integers value in the box to its right, and only displays the hits that give the worst deviations for the dimension. For example, if you type 3 in the box, the POINTINFO command only displays the three worst deviations.

Deviation Above - This checks the integer value in the box to its right, and only displays the hits that give the worst deviations for the dimension. For example, if you type 3 in the box, the POINTINFO command only displays the three worst deviations.

Out of Tolerance - This only displays the hits that have deviations that are out of tolerance. For hits related to features (not related to dimensions), only those hits with deviations larger than the Show Deviations Tolerance on the Setup Options dialog box's General tab are displayed. (See "Show Deviations Tolerance" in the "Setting Your Preferences" chapter.)

Min/Max - This only shows those hits that are the maximum and minimum deviation values for the dimension. For an example of MaxMin values, see the "Parameter Settings: Dimension tab" topic of the "Setting Your Preferences" chapter.