miim

### MP-524 RS-232 PH9/PH10 interface failure

See the following:

- Diagnostics on the MP RS-232 interface board port 0 failed.

The board may have failed or may not be installed in the MP.

- On an MP-30 system, diagnostics on the MP RS-232 interface board port 0 failed.

The board may have failed or may not be installed in the MP.

On an SMP system, diagnostics on the PH9/PH10 RS232 interface on the DCC card has failed.

For more information, see "MP Error Codes".

You should contact your Giddings & Lewis service representative.