core

#### Graphical Representation of Scan Vectors

When setting up the start, direction, and end points of the scan, PC-DMIS allows you to see a graphical representation of the initial touch vector, the direction vector, and the vector that is normal to the boundary plane where the scan will stop.

These vectors are shown as blue, green, and orange colored arrows in the Graphic Display area of your part.

Colored arrows showing vectors

Vectors and their graphical representations are:

- Initial Touch: Blue arrow

- Direction: Green arrow

- Boundary Plane: Orange arrow

More:

Creating Auto Features: Introduction

Quick Ways to Create Auto Features

Standardized Vector Sizing

Graphical Representation of Auto Feature and QuickFeature Vectors